



**Specifications:**

Voltage: 24V

Wattage: 1.85 W

Beam Angle: 100°

Kelvin: Natural White 4000K/ Cool White 6000K

Lumens: 100 lm

Finish: Stainless Steel

Cable Length: 1.5 meters

Life span: 30,000 hours

Cri/Ra: 80

**Product Code:**

IL300NW/CW

**Accessories:**

IL101: Intuition 24V 15W LED Driver with 6 Port Block

IL102: Intuition 24V 30W LED Driver with 12 Port Block

IL103: Intuition 24V 60W LED Driver with 12 Port Block

IL900: 2.5M CABLE extension for driver

**Dimensions:** Circumference: 67mm

Cut out size 48mm

Surface housing diameter: 67mm

Recessed light diameter: 65mm

Thickness of recessed light: 11mm

**Wiring Diagram:**

**Key Selling Points:**

* Product supplied with outer housing to enable surface lighting mounted
* LEDs are diffused by a frosted cover, for a more solid and pleasing lighting effect, whilst maintaining high light output. No visible dots.
* Stainless Steel fitting available in Natural White or Cool White.
* Direct replacement for Halogen under cabinet recess/surface light.
* Long lamp life
* Over 90% less energy used than Halogen – save money on your electric bills.